,Model##OTHER##,Test device##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Luminious flux with supply (lm)##OTHER##,Luminious flux in emrgency (lm)##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Description##OTHER##,Reference##OTHER##,Installation instructions##OTHER##,Color##OTHER##,Neck Material##OTHER##,Body Material##OTHER##,Bottom Cover Material##OTHER##
LINEAR 2N30 A (220-230) - B - Cool White LED,LINEAR 2N30 A,AutoTest,220,220,220,6000,"3 phase electrified track-mounted emergency luminaire. Rectangular body with rounded edges made of aluminium and synthetic material. Includes a connector/adapter that remains hidden inside the track. LiFePO4 batteries with electronics to control charging according to temperature, and independent voltage control for each module. An internal microprocessor checks the status of the device and periodically performs functionality and autonomy tests and reports the status using the two LED indicator lights that it includes.",-,"https://www.daisalux.com/en-us/pages/productos/fichas/frefunica.aspx?DB=DaisaluxProEn&CodProd=647644&CodsAcaPro=21744,12144,58&refB=LINEAR+2N30+A+(B)",White,Daisalux-Metal-Aluminium-White,Daisalux-Metal-Aluminium-White,Daisalux-Metal-Aluminium-White
LINEAR 2N30 A (220-230) - N - Cool White LED,LINEAR 2N30 A,AutoTest,198,198,198,6000,"3 phase electrified track-mounted emergency luminaire. Rectangular body with rounded edges made of aluminium and synthetic material. Includes a connector/adapter that remains hidden inside the track. LiFePO4 batteries with electronics to control charging according to temperature, and independent voltage control for each module. An internal microprocessor checks the status of the device and periodically performs functionality and autonomy tests and reports the status using the two LED indicator lights that it includes.",-,"https://www.daisalux.com/en-us/pages/productos/fichas/frefunica.aspx?DB=DaisaluxProEn&CodProd=647644&CodsAcaPro=21744,12144,58&refB=LINEAR+2N30+A+(B)",Black,Daisalux-Metal-Aluminium-Black,Daisalux-Metal-Aluminium-Black,Daisalux-Metal-Aluminium-Black
LINEAR 2N30 A (220-230) - NBN - Cool White LED,LINEAR 2N30 A,AutoTest,220,220,220,6000,"3 phase electrified track-mounted emergency luminaire. Rectangular body with rounded edges made of aluminium and synthetic material. Includes a connector/adapter that remains hidden inside the track. LiFePO4 batteries with electronics to control charging according to temperature, and independent voltage control for each module. An internal microprocessor checks the status of the device and periodically performs functionality and autonomy tests and reports the status using the two LED indicator lights that it includes.",-,"https://www.daisalux.com/en-us/pages/productos/fichas/frefunica.aspx?DB=DaisaluxProEn&CodProd=647644&CodsAcaPro=21744,12144,58&refB=LINEAR+2N30+A+(B)",Black-White-Black,Daisalux-Metal-Aluminium-Black,Daisalux-Metal-Aluminium-White,Daisalux-Metal-Aluminium-Black
LINEAR 2N30 A (220-230) - NBB - Cool White LED,LINEAR 2N30 A,AutoTest,220,220,220,6000,"3 phase electrified track-mounted emergency luminaire. Rectangular body with rounded edges made of aluminium and synthetic material. Includes a connector/adapter that remains hidden inside the track. LiFePO4 batteries with electronics to control charging according to temperature, and independent voltage control for each module. An internal microprocessor checks the status of the device and periodically performs functionality and autonomy tests and reports the status using the two LED indicator lights that it includes.",-,"https://www.daisalux.com/en-us/pages/productos/fichas/frefunica.aspx?DB=DaisaluxProEn&CodProd=647644&CodsAcaPro=21744,12144,58&refB=LINEAR+2N30+A+(B)",Black-White-White,Daisalux-Metal-Aluminium-Black,Daisalux-Metal-Aluminium-White,Daisalux-Metal-Aluminium-White
LINEAR 2N30 DALI (220-230) - B - Cool White LED,LINEAR 2N30 DALI,DALI,220,220,220,6000,"3 phase electrified track-mounted emergency luminaire. Rectangular body with rounded edges made of aluminium and synthetic material. Includes a connector/adapter that remains hidden inside the track. LiFePO4 batteries with electronics to control charging according to temperature, and independent voltage control for each module. An internal microprocessor checks the status of the device and periodically performs tests of functionality and autonomy and informs of the status. Suitable for connection to DALI control unit (IEC 62386-202 Ed.1: Digital addressable lighting interface - Part 202: Particular requirements for control gear - Self-contained emergency lighting device type 1). Suitable only for three-phase tracks with communication.",-,"https://www.daisalux.com/en-us/pages/productos/fichas/frefunica.aspx?DB=DaisaluxProEn&CodProd=647664&CodsAcaPro=21744,12144,58&refB=LINEAR+2N30+DALI+(B)",White,Daisalux-Metal-Aluminium-White,Daisalux-Metal-Aluminium-White,Daisalux-Metal-Aluminium-White
LINEAR 2N30 DALI (220-230) - N - Cool White LED,LINEAR 2N30 DALI,DALI,198,198,198,6000,"3 phase electrified track-mounted emergency luminaire. Rectangular body with rounded edges made of aluminium and synthetic material. Includes a connector/adapter that remains hidden inside the track. LiFePO4 batteries with electronics to control charging according to temperature, and independent voltage control for each module. An internal microprocessor checks the status of the device and periodically performs tests of functionality and autonomy and informs of the status. Suitable for connection to DALI control unit (IEC 62386-202 Ed.1: Digital addressable lighting interface - Part 202: Particular requirements for control gear - Self-contained emergency lighting device type 1). Suitable only for three-phase tracks with communication.",-,"https://www.daisalux.com/en-us/pages/productos/fichas/frefunica.aspx?DB=DaisaluxProEn&CodProd=647664&CodsAcaPro=21744,12144,58&refB=LINEAR+2N30+DALI+(B)",Black,Daisalux-Metal-Aluminium-Black,Daisalux-Metal-Aluminium-Black,Daisalux-Metal-Aluminium-Black
LINEAR 2N30 DALI (220-230) - NBN - Cool White LED,LINEAR 2N30 DALI,DALI,220,220,220,6000,"3 phase electrified track-mounted emergency luminaire. Rectangular body with rounded edges made of aluminium and synthetic material. Includes a connector/adapter that remains hidden inside the track. LiFePO4 batteries with electronics to control charging according to temperature, and independent voltage control for each module. An internal microprocessor checks the status of the device and periodically performs tests of functionality and autonomy and informs of the status. Suitable for connection to DALI control unit (IEC 62386-202 Ed.1: Digital addressable lighting interface - Part 202: Particular requirements for control gear - Self-contained emergency lighting device type 1). Suitable only for three-phase tracks with communication.",-,"https://www.daisalux.com/en-us/pages/productos/fichas/frefunica.aspx?DB=DaisaluxProEn&CodProd=647664&CodsAcaPro=21744,12144,58&refB=LINEAR+2N30+DALI+(B)",Black-White-Black,Daisalux-Metal-Aluminium-Black,Daisalux-Metal-Aluminium-White,Daisalux-Metal-Aluminium-Black
LINEAR 2N30 DALI (220-230) - NBB - Cool White LED,LINEAR 2N30 DALI,DALI,220,220,220,6000,"3 phase electrified track-mounted emergency luminaire. Rectangular body with rounded edges made of aluminium and synthetic material. Includes a connector/adapter that remains hidden inside the track. LiFePO4 batteries with electronics to control charging according to temperature, and independent voltage control for each module. An internal microprocessor checks the status of the device and periodically performs tests of functionality and autonomy and informs of the status. Suitable for connection to DALI control unit (IEC 62386-202 Ed.1: Digital addressable lighting interface - Part 202: Particular requirements for control gear - Self-contained emergency lighting device type 1). Suitable only for three-phase tracks with communication.",-,"https://www.daisalux.com/en-us/pages/productos/fichas/frefunica.aspx?DB=DaisaluxProEn&CodProd=647664&CodsAcaPro=21744,12144,58&refB=LINEAR+2N30+DALI+(B)",Black-White-White,Daisalux-Metal-Aluminium-Black,Daisalux-Metal-Aluminium-White,Daisalux-Metal-Aluminium-White
